| Emergency Power Supply (Standby Generator) History Card |
| --- |
| Refer to Standards – Signalling – SPS 26 Mains Failure Plant & SMP 42 Work on Signalling Power Supplies & ESM-26-02/03/04 Maintenance Schedules: SS 09 11 02 01, SS 09 11 02 02, SS 09 11 02 03 |
|  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **LOCATION:** |  |  |  |  |

|  |
| --- |
| |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | Date of Visit |  |  |  |  |  |  |  |  |  |  |  |  | | Emergency Supply Volts |  |  |  |  |  |  |  |  |  |  |  |  | | Start Battery Volts (Float V) |  |  |  |  |  |  |  |  |  |  |  |  | | Hour Meter Reading at Finish |  |  |  |  |  |  |  |  |  |  |  |  | | Battery SAE |  |  |  |  |  |  |  |  |  |  |  |  | | Indication on ELD  (with motor gen on line) |  |  |  |  |  |  |  |  |  |  |  |  | | BX reading to Earth |  |  |  |  |  |  |  |  |  |  |  |  | | NX reading to Earth |  |  |  |  |  |  |  |  |  |  |  |  | | Frequency |  |  |  |  |  |  |  |  |  |  |  |  | | Comments |  |  |  |  |  |  |  |  |  |  |  |  | | Name |  |  |  |  |  |  |  |  |  |  |  |  | | Signature |  |  |  |  |  |  |  |  |  |  |  |  | |
| *Note: 1) Where a reliable 120V ELD is fitted the operation of the ELD must be observed and tested under both normal and emergency power operation.* |
|  |