# ULTRASONIC FLAW DETECTOR CALIBRATION RECORD

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | |
| 12 MONTHLY ULTRASONIC FLAW DETECTOR CALIBRATION RECORD | | | | | | |
| Machine Identification: | | UT | | | | |
| UT Machine Type: | |  | | | | |
| Minder: | |  | | | | |
| Calibrated to: | |  | | | | |
|  | | | | | | |
| TEST DATE | RESULTS PASS/FAIL | | TESTED BY | RECORDED MEASUREMENT | | |
| HORIZONTAL | VERTICAL | OSG |
|  |  | |  |  |  |  |
|  |  | |  |  |  |  |
|  |  | |  |  |  |  |
|  |  | |  |  |  |  |
|  |  | |  |  |  |  |
|  |  | |  |  |  |  |
|  |  | |  |  |  |  |
|  |  | |  |  |  |  |
|  |  | |  |  |  |  |
|  |  | |  |  |  |  |
|  |  | |  |  |  |  |