# ULTRASONIC FLAW DETECTOR CALIBRATION RECORD

|  |
| --- |
|  |
| 12 MONTHLY ULTRASONIC FLAW DETECTOR CALIBRATION RECORD |
| Machine Identification: | UT |
| UT Machine Type: |  |
| Minder: |  |
| Calibrated to: |  |
|  |
| TEST DATE | RESULTSPASS/FAIL | TESTED BY | RECORDED MEASUREMENT |
| HORIZONTAL | VERTICAL | OSG |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |